{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["INÍCIO","INÍCIO_DIM","INÍCIO_DIM_COB","INÍCIO_DIM_INT","INÍCIO_DIM_SEC","INÍCIO_DIM_PAR","MODULO I"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":27,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"INÍCIO","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"INÍCIO_DIM","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"INÍCIO_DIM_COB","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"INÍCIO_DIM_INT","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"INÍCIO_DIM_SEC","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"INÍCIO_DIM_PAR","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"MODULO I","index":6,"n_rows":33,"n_cols":22,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tipo de cobertura","Material","n"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uma água","Plástico",1.0999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duas águas","Fibrocimento",1.0999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Quatro águas","Aço",1.0999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Metais não-ferrosos",1.0999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Intensidade de chuva","Ferro fundido",1.2E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Equação de intensidade","Concreto alisado",1.2E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Intensidade estimada","Alvenaria revestida",1.2E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cerâmica"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Seção da calha","Concreto não-alisado",1.2999999999999999E-2,null,null,840]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Retangular","Alvenaria de tijolos não-revestida",1.4999999999999999E-2,null,null,150]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Trapezoidal",null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Triangular"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Semicircular","SOLVER PARA RETANGULAR","Valor",null,"Inclinação",5.0000000000000001E-3,{"$f":"U15^(1/2)","v":7.0710678118654752E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n",1.2E-2,null,"n",1.0999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inclinação","inclinação",5.0000000000000001E-3,null,"Lamina",7.8014903151390494E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0,5%","lamina",{"$f":"R19/2","v":0},null,"largura",{"$f":"U17*2","v":0.15602980630278099}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.01,"base",0,null,"área molhada",{"$f":"U18*U17","v":1.2172650227441677E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,"m",null,null,0.02,"Área molhada",{"$f":"R19*R18","v":0},null,"Perímetro molhado",{"$f":"U17+U17+U18","v":0.31205961260556198}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Perimetro molhado",{"$f":"R19+R18+R18","v":0},null,"Raio hidráulico",{"$f":"U19/U20","v":3.9007451575695247E-2},{"$f":"U21^(2/3)","v":0.11501779884383043}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Curva","Raio Hidraulico",{"$f":"R20/R21","v":{"$error":"#DIV/0!"}},null,"Vazão de projeto",{"$f":"540","v":540}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sim","Vazão de projeto",1080,null,"Vazão calculada",{"$f":"60000*V15*V21*U19/U16","v":540.00000328103818}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Não","Vazão calculada",{"$f":"(60000/R16)*R20*(R22^(2/3))*(R17^(1/2))","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Diferença",{"$f":"R24-R23","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tipo de curva"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Canto arredondado"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Canto vivo"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Seção condutor vertical"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Circular"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Retangular"]